<font color=yellow>Screen Contents for a DM<font color=olive>_____________
<font color=silver>A screen for a diagnostic message (DM) shows the corresponding information received by a specific J1939 device. The device's address for the current view is shown in the DMxx info line. The line is yellow as long as the diagnostic message has been received within the last five seconds, otherwise it is white.<br>
<font color=yellow>>><font color=silver> Switch between diagnostic information received by different devices using the NEXT DEV hotkey.<br>
<br>
<font color=yellow>DM03 and DM11<font color=olive>________________________
<font color=silver>In contrast to viewing the information of diagnostic messages, using these two trigger the clearing of the diagnostic trouble codes (DTCs) on the J1939 network.<br>
<br>
<font color=yellow>Indicator Lamps (top line)<font color=olive>___________
<font color=silver>The line contains four indicator lamps which can have the statuses Off (gray), On, slowly blinking or quickly blinking.<br>
- MIL: Malfunction Indicator Lamp<br>
- RSL: Red Stop Lamp<br>
- AWL: Amber Warning Lamp<br>
- Prot: Protect Lamp<br>
<br>
<font color=yellow>REQUEST hotkey<font color=olive>_______________________
<font color=silver>Requests the diagnostic information of the diagnostic message indicated in the DMxx line from all J1939 devices.<br>
<br>
<font color=yellow>CLR LIST hotkey<font color=olive>______________________
<font color=silver>Clears the contents of the list. Afterwards the list is filled as the diagnostic message is received again.<br>
<br>
<font color=yellow>NEXT DEV hotkey<font color=olive>______________________
<font color=silver>Changes the view to the next 1939 device which has provided diagnostic information.<br>
