<font color=silver>Displays the measured amount of CAN traffic on the bus with a bar graph. Each vertical bar represents a sample interval. The average (yellow) and the maximum (red) busload result from the calculations within an interval. Optionally, the amount of CAN error frames can be viewed in a separate graph (blue).<br>
<br>
<font color=yellow>SETTINGS (Hotkey)<font color=olive>____________________
<font color=silver>Options to toggle between the view with and without display of the error rate and to do further settings.<br>
<br>
<font color=yellow>SAVE BMP (Hotkey)<font color=olive>____________________
<font color=silver>A screenshot named pict00000.bmp (sequential number) is written to the directory of the current project. The screenshot can be viewed later with the "View Files" main menu entry or downloaded via a USB connection.<br>
