<font color=silver>Record CAN traffic to a trace file on the internal memory card by pressing the START hotkey. The destination is automatically generated (from project directory, date, time) and indicated in the first three fields (Drive, Folder, File). You can adapt the file name to your own needs by clicking on it.<br>
<br>
<font color=yellow>Overwrite<font color=olive>____________________________
<font color=silver>If enabled, an already existing des-tination file is overwritten (usually when using own file names). Other-wise, an incremented number is appended to the file name.<br>
<br>
<font color=yellow>Max. size<font color=olive>____________________________
<font color=silver>Maximum size a trace file may have. If the size is reached during recor-ding, tracing is either stopped or continued in a new file (see "Multi file" setting).<br>
<br>
<font color=yellow>File format<font color=olive>__________________________
<font color=silver>- .trc (ASCII): The recording is done with the readable trace format 2.0 by PEAK-System.<br>
<font color=silver>- .btrc (binary): The recording is done with the memory-saving binary trace file format. This is the recom-mended format due to performance reasons. For further use on a PC, a conversion is necessary.<br>
<br>
<font color=yellow>Multi file<font color=olive>___________________________
<font color=silver>If enabled and the maximum file size is reached during recording, a new file is created with an incremented number in the file name. Otherwise, the recording is stopped.<br>
<br>
<font color=yellow>Trace options<font color=olive>________________________
<font color=silver>Different information types can be recorded:<br>
<font color=silver>- Data: regular CAN messages<br>
<font color=silver>- Errors: error frames<br>
<font color=silver>- Status: internal status messages<br>
