<font color=silver>Up to three areas are visible:<br>
- Incoming CAN messages<br>
- Transmit list (can be hidden)<br>
- Transmit sequences (can be hidden)<br>
The VIEW hotkey toggles the transmit areas.<br>
<br>
Use the push dial to move the selec-tion frame to one of the areas. The MENU hotkey provides specific func-tions for each area. Click on an area to access its entries. Use the BACK hotkey to leave this area again.<br>
<br>
The RESET hotkey clears the receive area and resets the internal CAN controller. The latter may be useful in case of CAN errors (Bus Off).<br>
<br>
<font color=yellow>Receive area (RxID)<font color=olive>__________________
<font color=silver>Select a message and press the MENU hotkey to change the location of this message in the list. Furthermore, a received message can be copied to the transmit list.<br>
<br>
<font color=yellow>Transmit list (TxID)<font color=olive>_________________
<font color=silver>Use the SETTINGS hotkey to load an already prepared transmit list. Use the MENU hotkey to edit an entry or add one to the transmit list.<br>
<br>
<font color=silver>NOTE: By default, changes in the transmit list are NOT saved. Change this behaviour via the SETTINGS hotkey.<br>
<br>
<font color=silver>The transmission of an entry with a given period can be enabled or dis-abled by clicking on it. Any entry can be transmitted once by using the SEND 1X hotkey.<br>
<br>
<font color=yellow>Transmit sequences<font color=olive>___________________
<font color=silver>The repeated transmission of an entry can be enabled or disabled by clic-king on it. Any entry can be trans-mitted once by using the SEND 1X hotkey.<br>
<br>
<font color=silver>NOTE: By default, changes in transmit sequences are NOT saved. Change this behaviour via the SETTINGS hotkey.<br>
