<font color=yellow>Green<font color=silver> course: CAN-High<br>
<font color=yellow>White<font color=silver> course: CAN-Low<br>
<font color=yellow>Blue<font color=silver> course:	difference<br>
<br>
<font color=yellow>Upper position bar<font color=olive>___________________
<font color=silver>- brown bar: the whole sample record<br>
<font color=silver>- yellow bar: current view in relation to the whole sample record<br>
<font color=silver>- red line: position of the trigger<br>
<br>
<font color=yellow>RX / TX<font color=olive>______________________________
<font color=silver>- brown courses: data communication between transceiver and CAN controller (violet: stuff bit)<br>
- blue lines: sample points used by the CAN controller<br>
<br>
<font color=yellow>Zoom<font color=olive>_________________________________
<font color=silver>Zoom the view in or out horizontally (time axis). The position bar on top gives an overview.<br>
<br>
<font color=yellow>H-pos<font color=olive>________________________________
<font color=silver>Shift the view horizontally (time axis). The position bar on top gives an overview.<br>
<br>
<font color=yellow>T=0<font color=olive>__________________________________
<font color=silver>Position the trigger to the pre-defined position on the screen (left, center, or right; see Settings).<br>
<br>
<font color=yellow>Cursor<font color=olive>_______________________________
<font color=silver>Enable and move Cursors 1 and 2 in order to measure periods.<br>
<br>
<font color=yellow>View<font color=olive>_________________________________
<font color=silver>Quickly toggle the displayed elements on the Scope screen.<br>
<br>
<font color=yellow>Single<font color=olive>_______________________________
<font color=silver>Wait once for a trigger event to record the signals.<br>
<br>
<font color=yellow>Run/Stop<font color=olive>_____________________________
<font color=silver>Repeatedly wait for a trigger event and record the signals until stopped manually.<br>
<br>
<font color=yellow>Report<font color=olive>_______________________________
<font color=silver>Show information about the CAN frame that has been decoded last from the signal course.<br>
<br>
<font color=yellow>Settings<font color=olive>_____________________________
<font color=silver>Change settings for the Scope function.<br>
<br>
<font color=yellow>Export<font color=olive>_______________________________
<font color=silver>Different information can be written to the internal memory card (configured in Settings): a screendump as bitmap, the Report as text, the contents of the sample buffer as CSV.<br>
<br>
<font color=yellow>Import<font color=olive>_______________________________
<font color=silver>Import a CSV file with sample buffer contents, e.g. from a previously done export.<br>
<br>
<font color=yellow>Bottom status bar<font color=olive>____________________
<font color=yellow>H<font color=silver>: horizontal display scale<br>
<font color=yellow>V<font color=silver>: vertical display scale<br>
<font color=yellow>Stopped/Waiting/Running<font color=silver>: status of the scope trigger<br>
<font color=yellow>C1/C2/CDiff<font color=silver>: time period measurements with cursors<br>
