<font color=yellow>1. <font color=silver>Make sure, there is CAN traffic on the connected CAN bus.<br>
<font color=yellow>2. <font color=silver>Select the CAN protocol being used on the CAN bus. TIP: If not sure, select "FD ISO" first.<br>
<font color=yellow>3. <font color=silver>Press the START hotkey to initiate the detection process. The predefined bit rates (see Settings entry "Bit rate" > "Edit") are tested. This can take several seconds.<br>
