<font color=olive>________________CAN__________________
<br>
<font color=yellow>Silent Startup<font color=olive>_______________________
<font color=silver>When the device is switched on, the set CAN bit rate is checked as to the traffic on the connected CAN bus. If the device's bit rate does not match, the device goes to listen-only mode to avoid impact by error frames (see also "Listen-only mode" below).<br>
<br>
<font color=yellow>Detect CAN bit rate<font color=olive>__________________
<font color=silver>Incoming CAN traffic is needed for this measurement. A predefined list of bit rates is used to check the bit rate setting.<br>
<br>
<font color=yellow>CAN protocol<font color=olive>_________________________
<font color=silver>Select the CAN protocol being used on the connected CAN bus, i.e. CAN 2.0 A/B ("Classic CAN"), CAN FD ISO 11898-1:2015, CAN FD non-ISO (first CAN FD implementation, for backwards compatibility). This does not refer to the Scope function which gathers information from the physical layer.<br>
<br>
<font color=yellow>Allow bit rate switch<font color=olive>________________
<font color=silver>If enabled, CAN FD frames can utilize the second (higher) bit rate for the data part.<br>
<br>
<font color=yellow>Bit rate<font color=olive>_____________________________
<font color=silver>Select one of the predefined CAN bit rates matching the one used by the connected CAN bus. If bit rate swit-ching is enabled for CAN FD (see setting above), the data bit rate must also match.<br>
<font color=silver>TIP: If you are not sure about the bit rate on the connected CAN bus, you may want to try the "Detect CAN bit rate" function above.<br>
<br>
<font color=yellow>Internal termination<font color=olive>_________________
<font color=silver>Activates the device-internal bus termination of 120 Ohms between CAN-High and CAN-Low lines. This is needed if the connected CAN bus only has one terminating resistor.<br>
<br>
<font color=silver>TIP: Use the menu command "Measurements > CAN Termination" to get information about the current total resistance.<br>
<br>
<font color=yellow>Listen-only mode<font color=olive>_____________________
<font color=silver>Shows what's going on, but doesn't affect traffic on the bus (especially CAN frame acknowledgements and error frames are not transmitted).<br>
<br>
<font color=yellow>Auto-reset on BusOff<font color=olive>_________________
<font color=silver>When the CAN controller has gone to BusOff error state due to many trans-mission errors, the PCAN-Diag FD automatically resets its CAN con-troller. This can come in handy e.g. in case of experiments with bit rates on other CAN nodes.<br>
<br>
<font color=olive>______________Display________________
<br>
<font color=yellow>Intro<font color=olive>________________________________
<font color=silver>When the PCAN-Diag FD is switched on, a splash screen can be shown for a few seconds before the main menu is brought onto the display. You can use a different splash screen for each project (see User Manual).<br>
<br>
<font color=yellow>Display orientation<font color=olive>__________________
<font color=silver>The orientation of the screen can be determined automatically or set to the following values:<br>
<font color=silver>0 portrait<br>
<font color=silver>90 landscape, controls right<br>
<font color=silver>180 portrait, upside down<br>
<font color=silver>270 landscape, controls left<br>
<br>
<font color=yellow>HDMI output<font color=olive>__________________________
<font color=silver>If enabled (default) and the PCAN-Diag FD is connected to an external display via HDMI/DVI cable, the display of the PCAN-Diag FD automa-tically switches to that external display. Disable to avoid the external display even if a physical connection is there.<br>
<br>
<font color=silver>NOTE: The PCAN-Diag FD uses a DVI signal for external display (compa-tible to HDMI). It has a resolution of 800 x 600 pixels and is delivered with 60 Hz.<br>
<br>
<font color=yellow>Screensaver timeout<font color=olive>__________________
<font color=silver>The display is dimmed after the PCAN-Diag FD device is not being used for the given period.<br>
<br>
<font color=yellow>Backlight intensity<font color=olive>__________________
<font color=silver>Adjust the brightness of the display here.<br>
<br>
<font color=olive>______________Device_________________
<br>
<font color=yellow>Pin 6 GND connection<font color=olive>_________________
<font color=silver>Connects the device's GND to pin 6 of the 9-pin D-Sub connector. For example, GND can be disconnected if you experience problems when searching a CAN signal with the scope function.<br>
<br>
<font color=yellow>Beeper<font color=olive>_______________________________
<font color=silver>The device gives acoustic feedback for several events. This can be turned off in general.<br>
<br>
<font color=yellow>Shutdown time (battery)<font color=olive>______________
<font color=silver>If operated with batteries, the device switches off after not being used for the given period. This function has no effect if the device is supplied by an external voltage.<br>
<br>
<font color=yellow>Date & time<font color=olive>__________________________
<font color=silver>The device's date and time can be set. Date and time are used when saving files to the internal memory card.<br>
<br>
<font color=yellow>Reset file index<font color=olive>_____________________
<font color=silver>File names for exported bitmaps or scope data include a number coming from a counter. The current counter state is shown in parentheses and can be reset to 0 by clicking "Reset".<br>
<br>
<font color=yellow>USB mode (reboot req.)<font color=olive>_______________
<font color=silver>NOTE: This option is only available on request for special purposes.<br>
<br>
<font color=yellow>USB auto-connect<font color=olive>_____________________
<font color=silver>If enabled, the PCAN-Diag FD auto-matically establishes a connection to the internal memory card as soon as a connection to a USB host on a PC or other device is detected. Otherwise, use the main menu entry "USB Connection".<br>
<br>
<font color=yellow>Exit options (hotkeys)<font color=olive>_______________
<font color=yellow>OK<font color=silver>: Use changes for this session only<br>
<font color=yellow>SAVE&OK<font color=silver>: Save changes until next Project change<br>
<font color=yellow>CANCEL<font color=silver>: Discard changes<br>
