<font color=silver>Measures the resistance between CAN-High and CAN-Low lines. The measure-ment does not affect the CAN commu-nication on the bus. Use the START hotkey for measurement.<br>
<br>
Both ends of a High-speed CAN bus must be terminated with 120-Ohm resistors. This results in a total resistance of 60 Ohms (two resistors in parallel).<br>
<br>
<font color=yellow>Int. CAN termination<font color=olive>_________________
<font color=silver>Depending on the CAN bus structure, the internal terminating resistor of 120 Ohms can be added.<br>
<font color=silver>NOTE: This setting is not saved permanently.<br>
<br>
<font color=yellow>Measured termination / Status<font color=olive>________
<font color=silver>While the measurement is running (see Status), the measuring value for the termination is updated about once per second.<br>
<br>
<font color=yellow>Calibration date<font color=olive>_____________________
<font color=silver>If a date is displayed, the measuring unit is calibrated. Otherwise from the main menu go to "Support > Calibration CAN Termination" and follow the instructions.<br>
