<font color=silver>Symbols to be transmitted are taken from the active symbol file (indica-ted on the bottom of the screen). Each Symbol definition renders an entry including the default values (for Period and Signal values). If not pre-defined, the values are 0.<br>
<br>
<font color=white>List of tasks<font color=silver>________________________
<font color=silver>* Toggle the periodical transission<br>
<font color=silver>> Click on the Symbol entry.<br>
<br>
<font color=silver>* Transmit once (if Period = 0)<br>
<font color=silver>> Click on the Symbol entry.<br>
<br>
<font color=silver>* Change a Symbol's cycle time<br>
<font color=silver>> Move selection frame to a Symbol entry and press EDIT hotkey.<br>
<br>
<font color=silver>* Change a Signal's value<br>
<font color=silver>> Move selection frame to a Signal entry and press EDIT hotkey.<br>
<br>
<font color=silver>* Collapse/expand Symbols<br>
<font color=silver>> Single Symbol entry: press push dial medium-long (1 sec.) on the Symbol entry.<br>
<font color=silver>> All Symbol entries: press and hold push dial.<br>
<br>
<font color=yellow>RESET (hotkey)<font color=olive>_______________________
<font color=silver>
<font color=silver>Rebuilds the Symbols list and resets the internal CAN controller. The latter may be useful in case of CAN errors (Bus Off).<br>
