<font color=yellow>Raw CAN Messages<font color=olive>_____________________
<font color=silver>Displays incoming message data in hexadecimal representation and pro-vides the possiblity to transmit single CAN messages or sequences.<br>
<br>
<font color=yellow>Receive Symbols<font color=olive>______________________
<font color=silver>Displays incoming message data in symbolic representation (with ID and receive counter). First, a symbol file must be applied via the Manage Symbols menu item.<br>
<br>
<font color=yellow>Transmit Symbols<font color=olive>_____________________
<font color=silver>Symbols from the applied symbol file (via the Manage Symbols menu item) can be transmitted onto the CAN bus with either predefined or edited values.<br>
<br>
<font color=yellow>Manage Symbols<font color=olive>_______________________
<font color=silver>Load a symbol file from the memory card and manage the display options for the symbolic view.<br>
<br>
<font color=yellow>Trace Messages<font color=olive>_______________________
<font color=silver>Record the CAN traffic (raw messages) to a file on the internal memory card.<br>
<br>
<font color=yellow>Play Back Trace<font color=olive>______________________
<font color=silver>Play back CAN messages onto the connected CAN bus from a previously recorded trace file or a prepared one.<br>
<br>
<font color=yellow>J1939<font color=olive>________________________________
<font color=silver>Function extension for diagnosing J1939 networks which is only available with a valid license file for the PCAN-Diag FD J1939 Add-in.<br>
