Notes for Use of Fujitsu Flash MCU Programmer for FMC-16LX

March 2010
Fujitsu Limited

This software writes data to flash memory contained in the Fujitsu microcontroller with flash memory
from a personal computer.

1.  System Requirements
	Personal computer:  IBM PC/AT compatibles with RS-232C port
	OS:  Japanese and English versions of Windows 2000 SP3, Windows XP SP2
	Memory:  Memory capacity more than OS requires
	Available disk space:  10 MB or more

	NOTICE:  The operations of all models that meet the above conditions may not be ensured.

2.  Explanation of Files Provided
	setup.exe:        Installer execution file
	Readme16LXe.txt:  Document file(english)
	Readme16LXj.txt:  Document file(japanese)

3.  Installation Procedure
3.1  Outline of Installer
	This installer includes the program for storage of installation information, called Windows 
	Installer.  Windows Installer is installed to the personal computer on which Windows 2000 or 
	earlier OS runs.  In this case, restart may be required.
	If the installation of Windows Installer is completed or Windows Installer has been preinstalled, 
	the installation of this software is started.  Before installation, be sure to uninstall the old
	version and reboot.

3.2  Setup Mode
	When Installer is started in the Setup mode, the window for the selection of "All" or "Custom"
	appears:
	"All" is the standard setup and should be selected.
	"Custom" should be selected only when setting the installation folder in a special place.
	Installation to a deep hierarchy of the folder may prevent Installer from operating.  The full
	path of the folder should be specified within 200 characters and the full path of the 8.3-format
	folder within 100 characters.
	When the operation is continued according to directions from Installer, the installation is 
	completed and the shortcut to this software is created as a program on the Start menu.

4. Uninstallation Procedure
	Open the "Start"-"Settings" "Control Panel" and start "Add/Remove Programs."  Select and 
	delete "FUJITSU FLASH MCU Programmer for FMC16LX."  After uninstallation, the 
	installation folder may be left.  In this case, delete the folder manually.  This software is 
	typically installed to Fujitsu\Fujitsu Flash MCU Programmer\FMC16LX below Program Files.  No 
	registry is used.

5. Cautions
	No operation of this software on the NEC PC98 series of personal computers is assured.
	This software is not intended for writing to mass-produced products.

Note:  Windows is the product name of Microsoft.



-------------------------------------------------------------------------------
History of update
V01L27
	m_flash.883C file add

V01L26
	add 883C
	add 931/S
	change Copy function interface
	add Check Sum function
	change Flash area display

V01L25
	add 884/A/B/C
	add 357A/AS/TA/TAS
	add 357E/ES/TE/TES

	cange chip name from 883 to 883/A/B

V01L24
	add 912,997,952,828B
	Caution change

V01L23
	add 923,924
	add 335
	add 962

	OS:Windows 2000 SP3, Windows XP SP2
	COM PORT 1-20

V01L22
	add 803
	The HELP file is corrected. 

V01L21
	operation on WindowsNT is no longer guaranteed.
	
	add 367E/ES/TE/TES

V01L20
	The HELP file is corrected. 

V01L19
	delete 16,25MHz-OSC for 395H.
	add 4,5,8MHz-OSC for 395H.
	add 922
	add 946A
	add 947A
	add 949A
	add 882

V01L18
	Version Change

V01L1881
	add 351/S
	add 351B/BS
	add 352B/BS

V01L1880
	add 883/884

V01L17
	add 342E/CE/ES/CES
	add 345E/CE/ES/CES
	add 346E/CE/ES/CES
	add 347E/CE/ES/CES
	add 349E/CE/ES/CES
	add 351E/ES/TE/TES
	add 352E/TES/TE/ES
	add 352A/TAS/TA/AS
	add 362E/ES/TE/TES
	add 867E/ES
	cange chip name from 347C/S/CS to 347A/CA/AS/CAS
	cange chip name from 351 to 351A/AS/TA/TAS
	cange chip name from 867 to 867A/AS
	delete 357/TAS/TA/AS
	delete 362
	delete 367

V01L16
	add 423GA/GC
	add 428GA/GC

V01L15
	add 357TAS/TA/AS

V01L14a
	add 334
	add 346A/CA/AS/CAS
	add 489
	add 983
	
V01L13a
	add 367
	add 362
	add 337
	add 351
	add 378
	add 395H
	cange chip name from 352/C/S/CS to 352/S
	delete 423GA/GB/GC.
	delete 428GA/GB/GC.
	internal Intel Hex decoder is added

V01L12
	add 342A/CA/AS/CAS
	add 345A/CA/AS/CAS
	add 349A/CA/AS/CAS
	add 488
	add 822
	add 823

V01L11
	add 352

V01L10
	add 334
	add 5,10MHz-OSC for MB90F347/C/S/CS
	add 5,10MHz-OSC for MB90F867
	CRC checking is added
	internal Motorola S decoder is added
	continuously writeing mode is deleted
	A temporary(binary) file is not created
	popup menu is changed

V01L09
	add 897/S

V01L08
	operation on windows95 is no longer guaranteed.

	add 438L/LS,439/S,455/S,456/S,457/S,347/C/S/CS,867
	add 804,498G
	add continuously write mode.
	chang chip name from 394 to 394/H.
	delete 16MHz-OSC for 387/S.
	delete 10,16,20MHz-OSC for 394/H.
	delete 8,16MHz-OSC for 423GA/GB/GC.
	delete 8,16MHz-OSC for 428GA/GB/GC.

V01L07
	change baudrate for 408,523,553,574,583,584,654.
	making temporary file in everytime.
	m_flash.428 add(lost in L06)
	chane DOWNLOAD sequence.

V01L06
	delete 328.
	cange chip name from 387 to 387/S
	cange chip name from 474 to 474H/L
	cange chip name from 591A to 591A/G


