<font color=silver>Shows incoming messages in symbolic re-presentation. The used symbol file is indicated in the status line on the bottom of the screen.<br>
<font color=yellow>>><font color=silver> Change the used symbol file and the displayed symbols via the previous-level menu item "Manage Symbols".<br>
<font color=yellow>>><font color=silver> Create a symbol file on a PC and transfer it onto this device with the supplied Windows software (PCAN Symbol Editor, PCAN-Diag FD Editor).<br>
<br>
<font color=silver>Symbols are shown with the affiliated CAN ID. Below each symbol, the con-tained variables with their values are shown. Enums and mulitplexers defined in the symbol file are taken into account for display.<br>
<font color=yellow>>><font color=silver> Click on an entry to fold or unfold its contents. Press and hold the push dial to fold or unfold all entries.<br>
<br>
<font color=silver>TIP: If you are missing a CAN message in the list, check the display set-tings for the used symbol file via the previous-level menu item "Manage Symbols > EditFile".<br>
<br>
<font color=silver>NOTE 1: Binary numbers (suffix 'b') are only shown up to 16 bits. If a number (i.e. variable) has more bits, it is automatically shown as decimal number.<br>
<br>
<font color=silver>NOTE 2: At this time, receive symbol definitions without given data length ("Valid for all Data Lengths") are not supported. Corresponding CAN messages are highlit red in the list.<br>
<br>
<font color=yellow>RESET (hotkey)<font color=olive>_______________________
<font color=silver>Clears the list of symbols, resets the symbol counters, and resets the internal CAN controller. The latter may be useful after a CAN error has been corrected and the bus status still is Bus Off (status display on the upper right).<br>
<br>
<font color=yellow>SORT PRNT (hotkey)<font color=olive>___________________
<font color=silver>Sorts the displayed symbols according to the selected element.<br>
<font color=silver>Press and hold (PRNT): A screenshot of the current view is saved to the project folder.<br>
<br>
<font color=silver>Changes in the list that would have influence on the sort order are not treated dynamically. To resort the list, select the sort command again.<br>
<br>
<font color=yellow>Transmit sequences<font color=olive>___________________
<font color=silver>Moving to this area is done by the GOTO TX hotkey.<br>
<font color=yellow>>><font color=silver> Click on a sequence entry to activate or deactivate its cyclic transmission.<br>
<font color=yellow>>><font color=silver> Press the SEND 1X hotkey to per-form a sequence transmission only once.<br>
