<font color=silver>With projects, the PCAN-Diag can quickly be adapted to different applications. A project contains different settings, CAN transmit lists, transmit sequences, and symbol files.<br>
<br>
<font color=yellow>Load Project<font color=olive>_________________________
<font color=silver>Select a project from the internal memory card to be loaded for work.<br>
<br>
<font color=silver>TIP: Use the provided Windows soft-ware PCAN-Diag FD Editor to create a project and transfer it to the PCAN-Diag FD.<br>
<br>
<font color=yellow>Save Project<font color=olive>_________________________
<font color=silver>If you have made changes to settings or transmit lists, you can save them for later use in the project file. This means that the changes are available even after loading another project in between.<br>
<br>
<font color=yellow>Create new Project<font color=olive>___________________
<font color=silver>On the internal memory card, a new project is created with a corres-ponding directory. This new project is used right away.<br>
<br>
<font color=yellow>Copy Project<font color=olive>_________________________
<font color=silver>Uses an existing project as template for a new one. In a first step, all projects on the internal memory card are presented for selection. In a second step, you can adapt the name for the new project. To use the new project, you need to load it.<br>
<br>
<font color=yellow>Delete Project<font color=olive>_______________________
<font color=silver>Deletes a selected project from the internal memory card. Afterwards it isn't available anymore on this device.<br>
<br>
<font color=yellow>Project<font color=olive> (bottom status bar)__________
<font color=silver>Shows the currently active project.<br>
