<font color=silver>The two pins 6 and 9 of the D-Sub connector may be used for additional supply purposes. Their voltage values (measuring range from -28 V to +28 V) can be monitored in a bar graph. The view of this graph can be adjusted via the SETTINGS hotkey.<br>
<br>
<font color=silver>NOTE: Pin 6 can be connected to GND internally. The setting is determined via the main "Settings" menu item.<br>
