<font color=yellow>Status line on top<font color=olive>___________________
<font color=silver>Shows:<br>
<font color=silver>- Power source<br>
<font color=silver>- Battery status<br>
<font color=silver>- TR for CAN transmission/reception<br>
<font color=silver>	* blinks during CAN traffic<br>
<font color=silver>	* yellow or red in case of errors<br>
<font color=silver>	* green otherwise<br>
<font color=silver>- Current time<br>
<br>
<font color=yellow>CAN Data<font color=olive>_____________________________
<font color=silver>Receive and transmit CAN messages, including symbolic display, transmit lists, and transmit sequences. Record incoming CAN traffic to a trace file and play it back later.<br>
<br>
<font color=yellow>Scope<font color=olive>________________________________
<font color=silver>Dual-channel oscilloscope specialized to CAN applications; with message decoding from the signal course (independent of CAN controller).<br>
<br>
<font color=yellow>Measurements<font color=olive>_________________________
<font color=silver>CAN-related measurements: bus load, bus termination (resistance), volta-ges at the D-Sub connector.<br>
<br>
<font color=yellow>Projects<font color=olive>_____________________________
<font color=silver>Load settings for the device, the scope, and measurements. Transmit lists, transmit sequences, and links to the used symbol files are inclu-ded. New projects can also be created.<br>
<font color=silver>The name of the currently used pro-ject is shown in the status line on the bottom.<br>
<br>
<font color=yellow>Settings<font color=olive>_____________________________
<font color=silver>Adjust hardware parameters for the CAN interface, the power management, and others. These settings are project-specific.<br>
<br>
<font color=yellow>USB Connection<font color=olive>_______________________
<font color=silver>Activate the USB connection between the internal memory card and the PC's operating system.<br>
<font color=silver>NOTE: This menu item is not available if "USB autoconnect" is enabled in the Settings.<br>
<br>
<font color=yellow>View Files<font color=olive>___________________________
<font color=silver>Take a look at images and text files, e.g. previously made screenshots or reports.<br>
<br>
<font color=yellow>Support<font color=olive>______________________________
<font color=silver>Functions that are used for mainte-nance, e.g. hardware information, firmware update, charge level reset.<br>
<br>
<font color=yellow>Help<font color=olive>_________________________________
<font color=silver>TIP: In many places, you can access the help text by pressing and holding hotkey 4.<br>
<br>
<font color=yellow>Power Off (with Lock Switch)<font color=olive>_________
<font color=silver>Switch off the device, optionally with enabling the power-on lock on the rear of the device (battery discharge avoidance).<br>
<br>
<font color=yellow>Status line on bottom<font color=olive>________________
<font color=silver>Shows the name of the currently used project.<br>
<br>
<font color=lime>Contact Information<font color=green>__________________
<font color=silver>PEAK-System Technik GmbH<br>
<font color=silver>Darmstadt, Germany<br>
<font color=silver>Phone: +49 6151 8173-20<br>
<font color=silver>E-mail: info@peak-system.com<br>
<font color=silver>Web: www.peak-system.com<br>
