<font color=yellow>Start scene<font color=olive>____________________________
<font color=silver>If checked, the scene that is selected in the next menu item is shown after device startup.<br>
<br>
<font color=yellow>Select scene<font color=olive>___________________________
<font color=silver>If the previous item is checked, select a scene file (*.ins or *.inp) for startup here.<br>
<br>
<font color=yellow>Start tracer<font color=olive>___________________________
<font color=silver>If checked, recording a trace is star-ted after device startup.<br>
<br>
<font color=red>NOTE:<font color=silver> Either a scene or the tracer can be active, not both at the same time.<br>
<br>
<font color=yellow>Tracer timeout<font color=olive>_________________________
<font color=silver>If after startup the tracer is active and does not receive a CAN message within the given time, it is stopped and the device is shut down. This function is disabled if set to "Never".<br>
<br>