<font color=yellow>File<font color=olive>___________________________________
<font color=silver>Shows the automatically generated name of the trace file that will be used for the next messages trace.<br>
<br>
<font color=yellow>Trace CAN 1/2<font color=olive>__________________________
<font color=silver>Shows settings for recording to a trace file on the memory card. The following settings are available: Off (no record-ing), Data (CAN data), Errors (error frames), and Data+Err. (CAN data and error frames).<br>
<br>
<font color=yellow>Trace file size<font color=olive>________________________
<font color=silver>This option is used to limit the maximum file size of a recording from 10 Mbyte up to 1 GByte.<br>
<br>
<font color=yellow>Trace timeout<font color=olive>__________________________
<font color=silver>If no CAN message is received within this time span, the device switches to sleep mode. To restart the device, a keystroke or a wake-up via the CAN bus is required. The Never entry keeps the tracer running.<br>
<br>
<font color=yellow>Multi file trace<font color=olive>_______________________
<font color=silver>If this option is active, the recording is saved to multiple files. If the maximum size of the trace file is reached, the recording is continued in a new file. If the option is inactive, the recording is stopped, when reaching the maximum file size.<br>
<br>
<font color=yellow>Trace type<font color=olive>_____________________________
<font color=silver>This determines the type of recording:<br>
- linear: The recording is progressive.<br>
- circular: A certain number of trace files is created while recording. If the maximum number of files is reached, the oldest is deleted and the index of all other files is reduced by 1.<br>
<br>
<font color=yellow>File count circular<font color=olive>____________________
<font color=silver>This value indicates the maximum number of trace files that are created for a recording of the Trace type circular.<br>
<br>
<font color=yellow>Session type<font color=olive>___________________________
<font color=silver>This setting determines whether the files created for a recording of the Trace type circular are overwritten or not.<br>
<br>
<font color=lime>Start<font color=green>__________________________________
<font color=silver>Starts the recording of messages. Note that CAN ID filtering may be enabled in the Device Settings.<br>
<br>
<br>
<font color=gray>Screen during recording<br>
<font color=gray>=======================================
<br>
<font color=yellow>Start time<font color=olive>_____________________________
<font color=silver>Specifies the start time of the recording.<br>
<br>
<font color=yellow>CAN queue level<font color=olive>________________________
<font color=silver>Current and maximum fill level of the receive queue. If the queue has reached a fill level of 100 percent, most likely some incoming CAN messages were not recorded.<br>
<br>
<font color=yellow>CAN messages total<font color=olive>_____________________
<font color=silver>Number of CAN messages that have been recorded.<br>
<br>
<font color=yellow>File size<font color=olive>______________________________
<font color=silver>Current size of the trace file in kByte and already used storage space relative to the maximum possible file size.<br>
<br>
<font color=yellow>File count<font color=olive>_____________________________
<font color=silver>Number of files recorded. When the recording is done with Trace type circular, the number is incremented linearly regardless of the current file index.<br>
<br>
<font color=yellow>Trace type<font color=olive>_____________________________
<font color=silver>Indicates the used trace type.<br>
<br>
<font color=yellow>Session type<font color=olive>___________________________
<font color=silver>Indicates the used session type.<br>
<br>